# Access to Eddie + + +

Start med: <https://alfresco.cimne.upc.edu/share/page/site/velassco/wiki-page?title=Access_to_UEDIN_VELaSSCo_dedicated_nodes>

Opprette VPN til Eddie:

<http://www.ed.ac.uk/information-services/computing/desktop-personal/vpn/vpn-l2tp-clients/vpn-l2tp-win7-manual>

# Logge på Eddie

Kontrollpanel\Alle kontrollpanelelementer\Nettverks- og delingssenter:

Koble til nettverk UoE L2TP VPN

Brukernavn: velassco

Ssh/Putty

eddie3.ecdf.ed.ac.uk, port 22

Olavs konto

Username: v1oliest

Password: Svanes\_123

Server EDM Lisens for VELaSSCo lic id: 10241, pwd: INRIA

# EDMsupervisor for Eddie databases

EDMsupervisor på windows. Connect via ssh tunnel.

1. Putty: Connection->SSH->Tunnels: 1) Source port: 9090, Destination: velassco-cluster02-ext.ecdf.ed.ac.uk:9090. 2) Source port: 9091, Destination: velassco-cluster02-ext.ecdf.ed.ac.uk:9091. This must be repeated for all appservers.
2. Putty: Connection: set hostname (velassco-cluster02-ext.ecdf.ed.ac.uk). press the Open button.
3. EDMsupervisor on Windows: create server context: tcp, localhost, 9090.

# velassco-cluster01…40

velassco-cluster01 and velassco-cluster02 have external addresses, which you can access via the University’s VPN. Their external addresses are:

velassco-cluster01-ext.ecdf.ed.ac.uk

velassco-cluster02-ext.ecdf.ed.ac.uk

You can only connect to velassco-cluster06…39 from velassco-cluser01 and possibly velassco-cluser02.

Export JOTNE\_DB=/exports/csce/datastore/eng/groups/velassco/jotne

# EDM licenses

In .bashrc: export EDM\_lic\_address=0123456789ab

EDM\_LIC\_650\_10241=xP3P,HOp.CUV0zdX\_'701m1plc4APVW.grr)&c'LEp3jDCmXGYMqQBf4Ntip7zRwrf&Tg(f2PRP/)d/JdoAA

EDM\_LIC\_602=jWE4XNuoL.q9A5u(bEwG\_52JZuV(htdsUhw5,CY/&s9AqVXku9IEgkC..lY-T4znGYZ7i-auRFK8I&Bx9Ota

# GID -> HBase

# GID -> EDMqueryManager

# VNC

# Lokal nett med ruter

Windows

Kontrollpanel\Alle kontrollpanelelementer\Nettverks- og delingssenter\Endre instillinger for nettverkskort->get

Egenskaper

TCP/IPv4 10.0.0.20

Linux

Nettverksinstillinger på ”kontakt” oppgasvelinje

Vired

Skiftenøkkel

IPv4

Adress: Manual (Automatisk DHCP tilbake)

10.0.0.21

Maske:

255.255.255.0